{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","م³/دقيقة","30","","","34"]
["","","التدفئة","منخفض جداً","م³/دقيقة","32","","","34"]
["","","","منخفض جداً","قدم مكعب في الدقيقة","1059","","","1200"]
["","","التدفئة","منخفض جداً","قدم مكعب في الدقيقة","1130","","","1200"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","550","550"]
["","","","العرض","mm","765","765","765","765"]
["","","","العمق","mm","285","285","285","285"]
["الوزن","الوحدة","","","kg","36","36","36","41"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","760","500","500","890"]
["","","التدفئة","منخفض جداً","rpm","820","320","320","890"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°مئوية مقياس الحوجلة الجافة","-10","-10","-10 (2)","-10"]
["","","","Max.","°مئوية مقياس الحوجلة الجافة","46","46","46 (2)","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","","46","46"]
["","","","Nom.","ديسيبل أمبير","48","","","46"]
["","Heating","","High","ديسيبل أمبير","","48","48"]
["","","","Nom.","ديسيبل أمبير","50","","","48"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","0.88","0.88","0.88","1.15"]
["","السعة","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","GWP","","","","675","675","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20","20 (1)","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","م","15","15.0","15.0","15"]
["","","IU - IU","Max.","م","7.5","7.5","7.5","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","30","30","30","30"]
["Standard Accessories","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","فولت","220-240","220-230-240","220-230-240","220-240"]
["Notes","","","","","","(1) - لغرفة واحدة"]
["","","","","","","","(1) - لغرفة واحدة"]
["","","","","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["Standard Accessories","Reducer assembly","","","","","","","1"]