{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B","4MXM80N2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","م³/دقيقة","24.1","24.1"]
["","","التدفئة","منخفض جداً","م³/دقيقة","24.1","24.1"]
["","","","منخفض جداً","cfm","851","851.0"]
["","","التدفئة","منخفض جداً","cfm","851.0","851.0"]
["الأبعاد","الوحدة","","الارتفاع","mm","734","734"]
["","","","العرض","mm","958","958"]
["","","","العمق","mm","340","340"]
["الوزن","الوحدة","","","كغ","63","67"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","48","49"]
["","Heating","","Nom.","ديسيبل أمبير","48","49"]
["سائل تبريد","النوع","","","","R-32","R-32"]
["","السعة","","","كغ","2.00","2.40"]
["","السعة","","","tCO2Eq","1.4","1.6"]
["","GWP","","","","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","25","25"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","15","15"]
["","","IU - IU","Max.","م","7.5","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","60","70"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","هرتز","50","50"]
["","Voltage","","","V","220-240","220-240"]