{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-A"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 3MXM52A2V1B","CHYHBH05AAV32 / 3MXM52A2V1B","CHYHBH05AFV32 / 3MXM68A2V1B","CHYHBH05AAV32 / 3MXM68A2V1B"]
["تسخين الماء الحار المنزلي","عام","","ملف تعريف الحمل المعلن عنه","","XL","","XL"]
["","المناخ المعتدل","","فئة فعالية طاقة تسخين الماء","","A","","A"]
["COP","","","","","4.49 (1)","4.49 (1)","3.91 (1)","3.91 (1)"]
["تدفئة المساحة","معدل مخرج الماء المناخي 55°مئوية","عام","Seasonal space heating eff. class","","A+","","A+"]
["","","","ηs (فعالية مساحة التدفئة الفصلية)","%","111.4","","113.3"]
["","","","SCOP","","2.86","","2.91"]
["Heating capacity","Nom.","","","كيلو واط","4.41 (1)","","4.50 (1)"]
["Notes","","","","","(1) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏=5‏° مئوية)، تجاوز المرجل","(1) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏=5‏° مئوية)، تجاوز المرجل","(1) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏=5‏° مئوية)، تجاوز المرجل","(1) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏=5‏° مئوية)، تجاوز المرجل"]
["Heating capacity","Nom.","","","كيلو واط","","4.41 (1)","","4.5 (1)"]
["تسخين الماء المنزلي","عام","","ملف تعريف الحمل المعلن عنه","","","XL","","XL"]
["","المناخ المعتدل","","فئة فعالية طاقة تسخين الماء","","","A","","A"]
["تدفئة المساحة","معدل مخرج الماء المناخي 55°مئوية","عام","SCOP","","","2.86","","2.91"]
["","","","فئة فعالية مساحة التدفئة الفصلية","","","A+","","A+"]