{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 5MXM-A9"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 5MXM90A2V1B9","CHYHBH08AAV32 / 5MXM90A2V1B9"]
["Heating capacity","Nom.","","","كيلو واط","4.5","6.78 (1)"]
["COP","","","","","4.04","4.17 (1)"]
["تسخين الماء المنزلي","عام","","ملف تعريف الحمل المعلن عنه","","XL","XL"]
["","المناخ المعتدل","","فئة فعالية طاقة تسخين الماء","","A","A"]
["تدفئة المساحة","معدل مخرج الماء المناخي 55°مئوية","عام","SCOP","","3.09","3.09"]
["","","","فئة فعالية مساحة التدفئة الفصلية","","A+","A+"]
["Notes","","","","","(1) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏=5‏° مئوية)، تجاوز المرجل","(1) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏=5‏° مئوية)، تجاوز المرجل"]