{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 2MXM-M"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M3V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M2V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM50M2V1B"]
["Cooling capacity","Nom.","","kW","3.0","3.00","3.00"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","302","302 (0.000)","310"]
["","نسبة فعالية استهلاك الطاقة","","","4.97","4.97","4.84"]
["","عامل الأداء","","","4.35","4.35","4.58"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A"]
["","","تدفئة","","A","A","A"]
["Heating capacity","Nom.","","kW","3.50","3.50"]
["Notes","","","","(1) - تستند استطاعات التبريد الإسمية إلى: درجة الحرارة الداخلية: 27‏°CDB، و19‏°CWB؛ درجة الحرارة الخارجية: 35‏°CDB، طول أنابيب سائل التبريد المكافئ: 5م، فرق المستوى: 0م. بيانات سلسلة الفعالية القياسية"]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Heating capacity","Min.","","kW","","","4.00"]
["Notes","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]