{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXS-L"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXS50L2V1B","FBA60A2VEB9 / RXS60L2V1B"]
["Cooling capacity","Nom.","","كيلو واط","","5.70"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","","826"]
["","نسبة فعالية استهلاك الطاقة","","","","3.45"]
["","عامل الأداء","","","","37.10"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A"]
["","","تدفئة","","","A"]
["Heating capacity","Nom.","","كيلو واط","","7.00"]
["Notes","","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["Outdoor unit","","","","RXS50L2V1B"]
["Cooling capacity","Nom.","","كيلو واط","5.00"]
["Heating capacity","Nom.","","كيلو واط","5.50"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.52"]
["","عامل الأداء","","","38.30"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي","710"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","كيلو واط","5.00"]
["","SEER","","","6.21"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","282"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","كيلو واط","4.40"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.06"]
["","Pdh استطاعة التدفئة عند -10°","","كيلو واط","3.73"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1517"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D"]