{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Outdoor unit","","","","AZAS71M2V1B"]
["Cooling capacity","Nom.","","kW","6.80"]
["Heating capacity","Nom.","","kW","7.50"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","6.80"]
["","SEER","","","5.57"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","427"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","4.50"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.81"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1654"]
["Notes","","","","(1) - التبريد: T2: درجة الحرارة الداخلية 26,6‏° مئوية CDB، و19,4‏° مئوية CWB، درجة الحرارة الخارجية 48°CDB [وحدة حرارية/ساعة/واط]"]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]