{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FBA50A2VEB / RXM50N2V1B","FBA60A2VEB / RXM60N2V1B"]
["Cooling capacity","Nom.","","kW","5.00","5.70"]
["تبريد المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","337"]
["","الاستطاعة","Pdesign","kW","","5.70"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","4.60"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","1,607"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","704","818"]
["","نسبة فعالية استهلاك الطاقة","","","3.55","3.48"]
["","عامل الأداء","","","3.83","3.71"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","A"]
["Heating capacity","Nom.","","kW","5.50","7.00"]
["Notes","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(2) - See separate drawing for electrical data","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A+"]
["","SEER","","","","5.91"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A+"]
["","SCOP/A","","","","4.01"]