{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ100C8VEB / RZQG100L9V1B","FBQ71C8VEB / RZQG71L9V1B","FBQ35C8VEB / FBQ35C8VEB / RZQG71L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQG100L9V1B","FBQ125C8VEB / RZQG125L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L9V1B","FBQ60C8VEB / FBQ60C8VEB / RZQG125L9V1B"]
["Cooling capacity","Nom.","","كيلوواط","9.5","6.8","","","","12.0"]
["تبريد المساحة","SEER","","","5.80","5.61, 6.11","5.10","5.10","5.10","5.81","5.10","5.10","5.10"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","574","390","467","652","652","723","824","824","824"]
["","الاستطاعة","Pdesign","كيلوواط","9.50","6.80","6.80","9.50","9.50","12.00","12.00","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","A+","A++","B","B","B","A+","B","B","B"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","11.30","6.00","6.00","11.30","11.30","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","4.61","4.01","3.80","3.80","3.80","4.21","3.80","3.80","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A++","A+","A","A","A","A+","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","3,432","2,095","2,211","4,164","4,164","4,227","4,683","4,683","4,683"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","1,220","970","","","","1,575"]
["","نسبة فعالية استهلاك الطاقة","","","3.89","3.50","","","","3.81"]
["","عامل الأداء","","","4.21","3.65","","","","3.83"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","","","","A"]
["","","تدفئة","","A","A","","","","A"]
["Heating capacity","Nom.","","كيلوواط","10.8","7.5","","","","13.5"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]