{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ50D2VEB / RXS50L2V1B","FBQ60D2VEB / RXS60L2V1B (Archived)"]
["Cooling capacity","Nom.","","كيلوواط","5.0 (2)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","710"]
["","نسبة فعالية استهلاك الطاقة","","","3.52 (1)"]
["","عامل الأداء","","","3.83 (1)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["Heating capacity","Nom.","","كيلوواط","5.50 (2)"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["Outdoor unit","","","","","RXS60L"]
["Cooling capacity","Nom.","","كيلوواط","","5.7"]
["Heating capacity","Nom.","","كيلوواط","","7.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","3.45"]
["","عامل الأداء","","","","3.71"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","","826"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","A"]
["","","تدفئة","","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A+"]
["","الاستطاعة","Pdesign","كيلوواط","","5.70"]
["","SEER","","","","5.86"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","340"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A+"]
["","الاستطاعة","Pdesign","كيلوواط","","4.60"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","4.01"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","1606"]