{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B8V1","FDBQ25B5V1"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","35.0","35.0"]
["","","","Low","ديسيبل أمبير","29.0","29.0"]
["","Cooling","","Low","ديسيبل أمبير","28.0","28.0"]
["","","","High","ديسيبل أمبير","35.0","35.0"]
["Standard Accessories","دليل التركيب والتشغيل","","","","1","1"]
["","مرشح هواء الشفط","","","","1","1"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35"]
["","غاز","","القطر الخارجي","mm","9.52"]
["","Drain","","","","27.2"]
["Sound power level","التبريد","","","ديسيبل أمبير","55","55"]
["","التدفئة","","","ديسيبل أمبير","55","55"]
["Dimensions","Unit","","العرض","mm","652","652"]
["","","","العمق","mm","502","502"]
["","","","الارتفاع","mm","230","230"]
["الغلاف","المادة","","","","Zinc coated low carbon steel","Zinc coated low carbon steel"]
["الوزن","الوحدة","","","كغ","17.0","17.0"]
["Fan","Air flow rate","التدفئة","High","م³/دقيقة","6.95"]
["","","","Low","م³/دقيقة","5.20"]
["","","التبريد","Low","م³/دقيقة","5.20"]
["","","","High","م³/دقيقة","6.50"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","هرتز","50","50"]
["","الاسم","","","","V1","V1"]
["","Voltage","","","V","230 +/-10%","230"]
["Notes","","","","","(1) - Sound values are measured in a semi-anechoic room.","(1) - يتم قياس قيم الصوت في غرفة شبه كاتمة للصدى."]
["","","","","","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت."]
["","","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]
["أنظمة التحكم","Wired remote control","","","","","BRC1D52, BRC1E52A/B"]
["Piping connections","Liquid","","القطر الخارجي","mm","","6.35"]
["","غاز","","القطر الخارجي","mm","","9.52"]
["","Drain","","","","","27.2"]