{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZAG100M7V1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZAG100M7V1B"]
["Cooling capacity","Nom.","","kW","9.50 (1)","9.50 (1)"]
["تبريد المساحة","SEER","","","8.00","8.60"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","416","387"]
["","الاستطاعة","Pdesign","kW","9.50","9.50"]
["","فئة فعالية استهلاك الطاقة","","","A++","A+++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","7.80","7.80"]
["","SCOP/A","","","4.48","4.51"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,438","2,421"]
["Heating capacity","Nom.","","kW","10.8 (2)","10.8 (2)"]
["Notes","","","","(1) - التبريد: T2: درجة الحرارة الداخلية 26,6‏° مئوية CDB، و19,4‏° مئوية CWB، درجة الحرارة الخارجية 48°CDB [وحدة حرارية/ساعة/واط]","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(4) - See separate drawing for electrical data"]