{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A8"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B8"]
["Cooling capacity","Nom.","","كيلو واط","5"]
["Heating capacity","Nom.","","كيلو واط","6"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.1"]
["","عامل الأداء","","","3.23"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","806"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","B"]
["","","تدفئة","","C"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","كيلو واط","5"]
["","SEER","","","5.84"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","300"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","كيلو واط","4.35"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.82"]
["","Pdh استطاعة التدفئة عند -10°","","كيلو واط","3.55"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1,594"]
["Notes","","","","(1) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["","","","","(2) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]