{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Cooling capacity","Nom.","","kW","3.40"]
["تبريد المساحة","SEER","","","6.24"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","191"]
["","الاستطاعة","Pdesign","kW","3.40"]
["","فئة فعالية استهلاك الطاقة","","","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","فئة فعالية استهلاك الطاقة","","","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","979"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","456"]
["","نسبة فعالية استهلاك الطاقة","","","3.73"]
["","عامل الأداء","","","4.08"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["Heating capacity","Nom.","","kW","4.00"]
["Notes","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Cooling capacity","Nom.","","kW","","5.00","5.70"]
["Heating capacity","Nom.","","kW","","6.00","7.20"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","3.21","3.29"]
["","عامل الأداء","","","","3.35","3.32"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي","","780","867"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","B","A"]
["","","تدفئة","","","C","C"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A+","A+"]
["","الاستطاعة","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","295","328"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A","A"]
["","الاستطاعة","Pdesign","kW","","4.35","4.71"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","3.86","3.87"]
["","Pdh استطاعة التدفئة عند -10°","","kW","","3.85","4.08"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","1578","1704"]