{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXS-L"]
[]
[]
[]
[]
["","","","","FHA50AVEB / RXS50L2V1B","FHA60AVEB / RXS60L2V1B"]
["Outdoor unit","","","","RXS50L2V1B","RXS60L2V1B"]
["Cooling capacity","Nom.","","كيلوواط","5.00","5.70"]
["Heating capacity","Nom.","","كيلوواط","6.00","7.20"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.27","3.31"]
["","عامل الأداء","","","3.35","3.32"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","765","861"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","C","C"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+","A+"]
["","الاستطاعة","Pdesign","كيلوواط","5.00","5.70"]
["","SEER","","","5.87","6.02"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","298","332"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A","A"]
["","الاستطاعة","Pdesign","كيلوواط","4.35","4.71"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.86","3.87"]
["","Pdh استطاعة التدفئة عند -10°","","كيلوواط","3.85","4.08"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1578","1705"]