{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXL-K"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXL35K2V1B","FHQ50CAVEB / RXL50K2V1B"]
["Cooling capacity","Min.","","كيلوواط","1.4","1.7"]
["","Max.","","كيلوواط","4.0","5.8"]
["","Nom.","","كيلوواط","3.40","5.00"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","475","785"]
["","نسبة فعالية استهلاك الطاقة","","","3.58","3.18"]
["","عامل الأداء","","","3.96","3.35"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","B"]
["","","تدفئة","","A","C"]
["Heating capacity","Nom.","","كيلوواط","4.00","6.00"]
["","Min.","","كيلوواط","1.3","1.6"]
["","Max.","","كيلوواط","5.1","6.8"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]