{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Sound pressure level","Heating","High","ديسيبل أمبير","46"]
["","","Silent operation","ديسيبل أمبير","30"]
["","","Low","ديسيبل أمبير","33"]
["","Cooling","Silent operation","ديسيبل أمبير","29"]
["","","Low","ديسيبل أمبير","32"]
["","","High","ديسيبل أمبير","38"]
["","","Nom.","ديسيبل أمبير","36"]
["","Cooling","Nom.","ديسيبل أمبير","35"]
["Standard Accessories","دليل التركيب","","","1"]
["","دليل التشغيل","","","1"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","1"]
["","بطاريات جافة قياس AAA","","","2"]
["","حامل جهاز التحكم عن بعد","","","1"]
["","لوح التثبيت","","","1"]
["","أنبوب عزل الحرارة (أنبوب سائل التبريد)","","","8"]
["","مرشح تنقية الهواء","","","1"]
["","مرشح إزالة الروائح بالتحفيز الضوئي","","","1"]
["","غطاء جانبي","","","2"]
["","رباط تحزيم","","","4"]
["أنظمة التحكم","Infrared remote control","","","ARC433B67"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35"]
["","غاز","القطر الخارجي","mm","9.5"]
["","Drain","","","18"]
["Sound power level","التبريد","","ديسيبل أمبير","53"]
["","التدفئة","","ديسيبل أمبير","59"]
["Dimensions","Unit","العرض","mm","1,050"]
["","","العمق","mm","200"]
["","","الارتفاع","mm","490"]
["الغلاف","اللون","","","Almond white"]
["الوزن","الوحدة","","kg","16"]
["Power supply","الطور","","","1~"]
["","Frequency","","هرتز","50"]
["","الاسم","","","VM"]
["","Voltage","","فولت","220-240"]
["Notes","","","","(1) - 220 فولت"]
["","","","","(2) - 230 فولت"]
["","","","","(3) - 240 فولت"]
["","","","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]