{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FNA35A2VEB9 / FNA35A2VEB9 / RZQSG71L3V1B","FNA35A2VEB9 / FNA35A2VEB9 / FNA35A2VEB9 / RZQSG100L9V1B","FNA50A2VEB9 / FNA50A2VEB9 / RZQSG100L9V1B","FNA35A2VEB9 / FNA35A2VEB9 / FNA35A2VEB9 / FNA35A2VEB9 / RZQSG125L9V1B","FNA50A2VEB9 / FNA50A2VEB9 / FNA50A2VEB9 / RZQSG125L9V1B","FNA60A2VEB9 / FNA60A2VEB9 / RZQSG125L9V1B"]
["Cooling capacity","Nom.","","كيلو واط","6.80","9.50","9.50","12.00","12.00","12.00"]
["تبريد المساحة","SEER","","","5.10","4.80","5.10","4.80","4.80","4.80"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","467","693","652","875","875","875"]
["","الاستطاعة","Pdesign","كيلو واط","6.80","9.50","9.50","12.00","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","A","B","A","B","B","B"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلو واط","6.00","7.10","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,211","2,616","2,800","2,800","2,800","2,800"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","","1,855","1,573","2,335","2,034","2,439"]
["","نسبة فعالية استهلاك الطاقة","","","3.15","2.56","3.02","2.57","2.95","2.46"]
["","عامل الأداء","","","","2.66","3.26","2.90","3.44","3.08"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","E","B","E","C","E"]
["","","تدفئة","","","E","C","D","B","D"]
["Heating capacity","Nom.","","كيلو واط","","10.80","10.80","13.50","13.50","13.50"]
["Notes","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]