{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","33.0","33.0","36.0","36.0"]
["","","","Nom.","ديسيبل أمبير","31.0","31.0","33.0","33.0"]
["","","","Low","ديسيبل أمبير","28.0","28.0","30.0","30.0"]
["","Cooling","","متوسط","ديسيبل أمبير","31.0","31.0","33.0","33.0"]
["","","","Low","ديسيبل أمبير","28.0","28.0","30.0","30.0"]
["","","","High","ديسيبل أمبير","33.0","33.0","36.0","36.0"]
["Control systems","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Piping connections","Liquid","","القطر الخارجي","مم","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","مم","9.52","9.52","12.7","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","التبريد","","","ديسيبل أمبير","53.0","53.0","56.0","56.0"]
["Dimensions","Unit","","العرض","مم","790","790","1,190","1,190"]
["","","","العمق","مم","200","200","200","200"]
["","","","الارتفاع","مم","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["","Colour","","","","Unpainted","Unpainted","Unpainted","Unpainted"]
["الوزن","الوحدة","","","كغ","23.0","23.0","30.0","30.0"]
["Fan","External static pressure","","عالٍ","باسكال","48","48","49","49"]
["","","","الإسمي","باسكال","30","30","40","40"]
["","Air flow rate","التدفئة","High","م³/دقيقة","8.7","8.7","16.0","16.0"]
["","","","Low","م³/دقيقة","7.3","7.3","13.5","13.5"]
["","","","Nom.","م³/دقيقة","8.0","8.0","14.8","14.8"]
["","","التبريد","Low","م³/دقيقة","7.3","7.3","13.5","13.5"]
["","","","Nom.","م³/دقيقة","8.0","8.0","14.8","14.8"]
["","","","High","م³/دقيقة","8.7","8.7","16.0","16.0"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","الاسم","","","","VE","VE","VE","VE"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - يتضمن أرجل التركيب","(1) - يتضمن أرجل التركيب","(1) - يتضمن أرجل التركيب","(1) - يتضمن أرجل التركيب"]
["","","","","","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]