{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXG-L"]
[]
[]
[]
[]
["","","","","FTXG20LV1BW / RXG20L2V1B","FTXG25LV1BW / RXG25L2V1B","FTXG35LV1BW / RXG35L2V1B","FTXG50LV1BW / RXG50L2V1B"]
["Cooling capacity","Min.","","كيلوواط","1.3","1.3","1.4","1.7"]
["","Max.","","كيلوواط","2.8","3.0","3.8","5.3"]
["Heating capacity","Min.","","كيلوواط","1.3","1.3","1.4","1.7"]
["","Max.","","كيلوواط","4.3","4.5","5.0","6.5"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.59","4.59","3.97","3.53"]
["","عامل الأداء","","","5.00","4.42","4.06","3.65"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","250.5","261.5","441","680"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A"]
["","","تدفئة","","A","A","A","A"]
["Piping connections","Drain","OD","مم","18","18.0","18.0","18.0"]
["وصلات الأنابيب","غاز","القطر الخارجي","مم","9.5","9.5","9.5","12.7"]
["","سائل","القطر الخارجي","مم","6.35","6.35","6.35","6.35"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+++","A+++","A++","A++"]
["","الاستطاعة","Pdesign","كيلوواط","2.30","2.40","3.50","4.80"]
["","SEER","","","8.52","8.50","7.00","6.70"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","94","99","175","251"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A+"]
["","الاستطاعة","Pdesign","كيلوواط","2.10","2.70","3.00","4.60"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.60","4.60","4.60","4.24"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","639","821","913","1519"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]