{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":14,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 4MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM25N2V1B / FTXM42N2V1B / 4MXM68A2V1B9","FTXM35N2V1B / FTXM35N2V1B / 4MXM68A2V1B9","FTXM20N2V1B / FTXM50N2V1B / 4MXM68A2V1B9","FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 4MXM68A2V1B9","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / 4MXM68A2V1B9","FTXM20N2V1B / FTXM20N2V1B / FTXM42N2V1B / 4MXM80A2V1B9","FTXM20N2V1B / FTXM25N2V1B / FTXM35N2V1B / 4MXM80A2V1B9","FTXM35N2V1B / FTXM42N2V1B / 4MXM80A2V1B9","FTXM20N2V1B / FTXM60N2V1B / 4MXM80A2V1B9","FTXM20N2V1B / FTXM20N2V1B / FTXM20N2V1B / FTXM20N2V1B / 4MXM80A2V1B9"]
["Cooling capacity","Nom.","","كيلو واط","6.7","6.8","6.8","6.8","6.5","8.00","7.40","7.70","7.40","7.40"]
["Heating capacity","Nom.","","كيلو واط","8.30","8.60","8.60","8.60","8.20","9.40","9.30","9.00","9.30","9.60"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.74","3.94","3.59","3.85","4.01","3.56","3.79","3.11","3.43","4.17"]
["","عامل الأداء","","","3.95","3.81","3.82","4.38","4.49","4.08","4.02","3.56","3.73","4.58"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","896","863","947","883","810","1125","977","1236","1079","887"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A","B","A","A"]
["","","تدفئة","","A","A","A","A","A","A","A","B","A","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","الاستطاعة","Pdesign","كيلو واط","6.70","6.80","6.80","6.80","6.50","8.00","7.40","7.70","7.40","7.40"]
["","SEER","","","6.94","6.97","6.75","7.71","7.76","6.93","7.07","6.52","6.73","7.40"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","338","342","352","309","294","405","370","417","387","351"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A","A+","A","A+","A+","A+","A+","A+","A+","A+"]
["","الاستطاعة","Pdesign","كيلو واط","4.30","4.80","4.50","5.30","5.30","5.37","5.37","4.27","4.27","6.23"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.86","4.00","3.90","4.10","4.09","4.34","4.31","4.23","4.33","4.56"]
["","Pdh استطاعة التدفئة عند -10°","","كيلو واط","3.41","3.73","3.55","4.22","4.21","4.34","4.37","3.68","3.71","4.73"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1559","1679","1612","1807","1814","1732","1744","1413","1382","1913"]