{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Cooling capacity","Nom.","","kW","4"]
["Heating capacity","Nom.","","kW","4.2"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.71"]
["","عامل الأداء","","","3.75"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي","539"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","kW","4"]
["","SEER","","","7.74"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","181"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","kW","3.2"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.3"]
["","Pdh استطاعة التدفئة عند -10°","","kW","2.46"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1041"]
["Notes","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["Cooling capacity","Nom.","","kW","","4.00"]
["Heating capacity","Nom.","","kW","","5.20"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","","554"]
["","عامل الأداء","","","","3.68"]
["","نسبة فعالية استهلاك الطاقة","","","","3.61"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A"]
["","","تدفئة","","","A"]