{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-G"]
[]
[]
[]
[]
["","","","","FTXS20G2V1B / RXS20G2V1B","FTXS25G2V1B / RXS25G2V1B","FTXS35G2V1B / RXS35G2V1B","FTXS42G2V1B / RXS42G2V1B","FTXS50G2V1B / RXS50G2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Max.","","kW","2.8","3.2","4.0","5.0","5.3"]
["","Nom.","","kW","2.0 (1)","2.5 (1)","3.5 (1)","4.2 (1)","5.0 (1)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","235","275","435","610","760"]
["","نسبة فعالية استهلاك الطاقة","","","4.26","4.55","4.02","3.44","3.29"]
["","عامل الأداء","","","4.29","4.53","4.17","3.67","3.69"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.7 (2)","3.4 (2)","4.0 (2)","5.4 (2)","5.8 (2)"]
["","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Max.","","kW","4.3","4.7","5.2","6.0","6.5"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]