{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L8Y1B","FUQ71CVEB / RZQG71L8Y1B","FUQ100CVEB / RZQG100L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG100L8Y1B","FUQ125CVEB / RZQG125L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG125L8Y1B"]
["Cooling capacity","Nom.","","كيلوواط","","6.8","9.5","","12.0"]
["تبريد المساحة","SEER","","","6.50","6.42","6.11","5.10","5.61","5.10"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","367","371","545","652","749","824"]
["","الاستطاعة","Pdesign","كيلوواط","6.80","6.80","9.5","9.50","12","12.00"]
["","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","B","A+","B"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","7.60","7.60","11.3","11.30","14.13","12.71"]
["","SCOP/A","","","4.20","4.20","4.5","3.80","4.44","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+","A+","A","A+","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,534","2,534","3,516","4,164","4,456","4,683"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","840","1,230","","1,770"]
["","نسبة فعالية استهلاك الطاقة","","","","4.05","3.86","","3.39"]
["","عامل الأداء","","","","4.08","3.95","","3.42"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A","A","","A"]
["","","تدفئة","","","A","A","","B"]
["Heating capacity","Nom.","","كيلوواط","","7.5","10.8","","13.5"]
["Notes","","","","","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","(2) - يتوافق SEER وSCOP مع EN 14825","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]