{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL1"]
[]
[]
[]
[]
["","","","","JEHCCU0135CL1"]
["الوزن","الوحدة","","kg","61"]
["Dimensions","Unit","العرض","mm","876"]
["","","العمق","mm","430"]
["","","الارتفاع","mm","606"]
["الغلاف","اللون","","","Light grey"]
["Fan","النوع","","","محوري"]
["Power supply","الطور","","","1~"]
["","Frequency","","Hz","50"]
["","Voltage","","V","230"]
["Notes","","","","(1) - SRG = 20 درجة مئوية، Ta = 32 درجة مئوية، Te = - 35 درجة مئوية"]
["","","","","(2) - يتم قياس مستوى ضغط الصوت عند 10م في غرفة عازلة"]
["","","","","(3) - وظيفتها تعتمد على غازات الاحتباس الحراري المفلورة"]