{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Type","","","","","جهاز تنقية الهواء"]
["Application","","","","","Floor standing type"]
["الغلاف","Colour","","","","White"]
["Dimensions","Unit","","الارتفاع","mm","500"]
["","","","العرض","mm","270"]
["","","","العمق","mm","270"]
["الوزن","الوحدة","","","كغ","6.8"]
["Applicable room area","m²","","","","41 (1), 82 (2)"]
["CADR","م³/ساعة","","","","320"]
["Air purifying operation","Power input","","Turbo","كيلو واط","0.037"]
["","","","M","كيلو واط","0.015"]
["","","","L","كيلو واط","0.010"]
["","","","Silent","كيلو واط","0.008"]
["Sound pressure level","Air purifying operation","","Turbo","ديسيبل أمبير","53"]
["","","","Medium","ديسيبل أمبير","39"]
["","","","Low","ديسيبل أمبير","29"]
["","","","Silent","ديسيبل أمبير","19"]
["Fan","Air flow rate","Air purifying operation","Turbo","م³/ساعة","330"]
["","","","Medium","م³/ساعة","192"]
["","","","Low","م³/ساعة","120"]
["","","","Silent","م³/ساعة","66"]
["Dust collecting method","","","","","مرشح HEPA إلكتروستاتيكي"]
["Deodorizing method","","","","","جريان سريع + محفز إزالة الروائح"]
["أجهزة السلامة","العنصر","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Standard Accessories","جهاز تحكم عن بعد","","","","1"]
["","حامل جهاز التحكم عن بعد","","","","1"]
["","مرشح HEPA إلكتروستاتيكي","","","","1"]
["","مرشح مزيل للروائح","","","","1"]
["","دليل التشغيل","","","","1"]
["Power cord","م","","","","1.8"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","هرتز","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Running current","Air purifying operation","","Turbo","A","0.32"]
["","","","Medium","A","0.14"]
["","","","Low","A","0.10"]
["","","","Silent","A","0.08"]
["Notes","","","","","(1) - منطقة الغرفة القابلة للتطبيق مناسبة لتشغيل الوحدة ذات أعلى سرعة للمروحة (HH). تُشير منطقة الغرفة القابلة للتطبيق إلى المساحة حيث يوجد كمية معينة من جسيمات الغبار والتي يمكن إزالتها خلال 30 دقيقة. (JEM 1467)"]
["","","","","","(2) - تم التحويل إلى معايير NRCC من قيم الاختبار وفقاً لـ JEM1467."]
["","","","","","(3) - تم التحويل إلى معايير CADR من قيم الاختبار وفقاً لـ JEM1467."]
["","","","","","(4) - مستويات صوت التشغيل هي عبارة عن متوسط قيم مقاسة على مسافة 1م أمام الوحدة وعلى يمينها ويسارها وأعلاها. (وهي تساوي القيم في غرفة عازلة للصوت)"]
["","","","","","(5) - مرشح HEPA الإلكتروستاتيكي مركب في الوحدة."]
["","","","","","(6) - وظيفة أخرى: وظيفة التشكيل النشط. وظيفة إعادة بدء التشغيل تلقائيًا"]