{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP60N5V1B9","RXP71N5V1B9"]
["الأبعاد","الوحدة","","الارتفاع","mm","556","556","556","734","734","734"]
["","","","العرض","mm","740","740","740","954","954","954"]
["","","","العمق","mm","343","343","343","401","401","401"]
["الوزن","الوحدة","","","kg","24","24","26","46","50","50"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10","-10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","48","48","48","48","48","48"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18","18","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","46","48"]
["","","","Nom.","dBA","","","","47","49","52"]
["","Heating","","High","dBA","47","47","48"]
["","","","Nom.","dBA","","","","49","49","52"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","0.55","0.55","0.70","0.9","1.15","1.15"]
["","السعة","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20","20","30","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","12","12","12","20","20","20"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Drain cap","","","","","","","3","3","3"]
["Notes","","","","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]