{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","734","734","734"]
["","","","العرض","mm","870","870","870"]
["","","","العمق","mm","373","373","373"]
["الوزن","الوحدة","","","كغ","52","52","52"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","62.0","63.0","64.0"]
["","التدفئة","","","ديسيبل أمبير","62.0","63.0","64.0"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","48.0","49.0","50.0"]
["","Heating","","Nom.","ديسيبل أمبير","48.0","49.0","50.0"]
["سائل تبريد","النوع","","","","","R-32"]
["","السعة","","","كغ","1.55","1.55","1.55"]
["","GWP","","","","675.0","675.0","675.0"]
["","السعة","","","tCO2Eq","1.05","1.05","1.05"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.50","12.7","12.7"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","50","50"]
["","","نظام","بدون شحن","م","30","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","30.0","30.0","30.0"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","","1~"]
["Power supply","Frequency","","","هرتز","50","50","50"]
["","Voltage","","","V","","220-240"]