{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":13,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NY1"]
[]
[]
[]
[]
["","","","","","RZAG71N2Y1B","RZAG71N7Y1B","RZAG100N7Y1B","RZAG100N2Y1B","RZAG125N7Y1B","RZAG125N2Y1B","RZAG140N7Y1B","RZAG140N2Y1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","870","870","870","870","870","870","870","870"]
["","","","العرض","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","العمق","mm","460","460","460","460","460","460","460","460"]
["الوزن","الوحدة","","","kg","81","81","85","85","94","94","94","94"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","52","52","52","52","52","52","52","52"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18","18","18","18","18","18"]
["مستوى طاقة الصوت","التبريد","","","dBA","64","64","66","66","69","69","70","70"]
["","التدفئة","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Sound pressure level","Cooling","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Heating","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","3.20","3.2","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["","السعة","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","10","10","10","10","10","10","10","10"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","55","55","85","85","85","85","85","85"]
["","","نظام","مكافئ","م","75","75","100","100","100","100","100","100"]
["","","","بدون شحن","م","40","40","40","40","40","40","40","40"]
["Piping connections","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual","See installation manual","See installation manual","See installation manual","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","م","30","30","30","30","30","30","30","30"]
["","","IU - IU","Max.","م","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["وحدة التزويد بالطاقة","الطور","","","","3~","3~","3~","3~","3~","3~","3~","3~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["تيار - 50 هرتز","قيمة الأمبير القصوى للفاصمة (MFA)","","","A","16","16","16","16","16","16","16","16"]
["Notes","","","","","","","","","(1) - حسب ENER Lot 21","(1) - حسب ENER Lot 21","(1) - حسب ENER Lot 21","(1) - حسب ENER Lot 21"]