{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKEQ"]
[]
[]
[]
[]
["","","","","EKEQFCBV3","EKEQMCBAV3","EKEQDCBV3","EKEQFCBAV3","EKEQMCBV3"]
["Outdoor unit","","","","ERQ","VRV","ERQ","ERQ","VRV"]
["Application","","","","Pair","Multi","Pair","Pair","Multi"]
["Dimensions","Unit","Height","mm","132","132","132","132","132"]
["","","Width","mm","400","400","400","400","400"]
["","","Depth","mm","200","200","200","200","200"]
["Weight","Unit","","kg","3.9","3.6","3.6","3.9","3.6"]
["Operation range","Cooling","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","Max.","°CDB","40","40","40","40","40"]
["Standard Accessories","Thermistor (R1T)","","","0","1","1","0","1"]
["","Thermistor (R2T/R3T)","","","2","2","2","2","2"]
["","Insulation sheet","","","2","2","2","2","2"]
["","Rubber sheet","","","2","2","2","2","2"]
["","Wire to wire splice","","","4","6","6","4","6"]
["","Installation and operation manual","","","1","1","1","1","1"]
["","Screw nut","","","7","9","8","7","9"]
["","Tie-wraps","","","6","6","6","6","6"]
["","Capacity setting adapter","","","7","8","7","7","8"]
["","Stopper (closing up)","","","2","0","0","2","0"]
["Power supply","Name","","","V3","V3","V3","V3","V3"]
["","Phase","","","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50","50"]
["","Voltage","","V","230","230","230","230","230"]