{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-R"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RXM35R5V1B","FBA50A2VEB9 / RXM50R2V1B","FBA50A2VEB9 / RXM50R5V1B","FBA60A2VEB9 / RXM60R2V1B","FBA60A2VEB9 / RXM60R5V1B"]
["Cooling capacity","Nom.","","kW","3.40","5.00","5.00","5.70","5.70"]
["Heating capacity","Nom.","","kW","4.00","5.50","5.50","7.00","7.00"]
["Nominal efficiency","Annual energy consumption","","kWh","423","704","704","819","819"]
["","COP","","","4.02","3.83","3.83","3.71","3.71"]
["","EER","","","4.02","3.55","3.55","3.48","3.48"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","191","279","279","336","336"]
["","Energy efficiency class","","","A++","A++","A++","A+","A+"]
["","Capacity","Pdesign","kW","3.40","5.00","5.00","5.70","5.70"]
["","SEER","","","6.23","6.27","6.27","5.91","5.91"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","996","1,517","1,517","1,607","1,607"]
["","Capacity","Pdesign","kW","2.90","4.40","4.40","4.60","4.60"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","","3.73","3.73","3.99","3.99"]
["","SCOP/A","","","4.07","4.06","4.06","4.01","4.01"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]