{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQSG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQSG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQSG125L8Y1B","FCAG125BVEB / RZQSG125L8Y1B","FCAG140BVEB / RZQSG140L7Y1B"]
["Cooling capacity","Nom.","","kW","9.5","9.5","12.0","12.0","13.4"]
["Heating capacity","Nom.","","kW","10.8","","","13.5","15.5"]
["Nominal efficiency","EER","","","3.30","3.20","2.91","2.91","2.40"]
["","COP","","","3.54","","","3.41","3.41"]
["","Annual energy consumption","","kWh","1,439","","","2,062"]
["","Energy labeling Directive","Cooling","","A","","","C"]
["","","Heating","","B","","","B"]
["Space cooling","Energy efficiency class","","","A++","A","B","A"]
["","Capacity","Pdesign","kW","9.50","9.50","12.00","12.00","13.40"]
["","SEER","","","6.50","5.10","4.80","5.30","6.18"]
["","Annual energy consumption","","kWh/a","512","652","875","793","1,300"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A","A","A+"]
["","Capacity","Pdesign","kW","7.60","7.60","7.60","8.03","11.56"]
["","SCOP/A","","","4.10","3.80","3.80","4.01","4.18"]
["","Annual energy consumption","","kWh/a","2,596","2,797","2,800","2,804","3,872"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]