{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXS50L2V1B","FDXM60F3V1B9 / RXS60L2V1B"]
["Cooling capacity","Min.","","kW","1.70","1.70"]
["","Max.","","kW","5.30","6.50"]
["","Nom.","","kW","5.00","6.00"]
["Space cooling","SEER","","","5.72","5.51"]
["","Annual energy consumption","","kWh/a","306","381"]
["","Capacity","Pdesign","kW","5.00","6.00"]
["","Energy efficiency class","","","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.00","4.60"]
["","SCOP/A","","","3.93","3.80"]
["","Energy efficiency class","","","A","A"]
["","Pdh Heating capacity at -10°","","kW","3.55","3.94"]
["","Annual energy consumption","","kWh/a","1,425","1,693"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","12.70","12.70"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","Annual energy consumption","","kWh","825","1,030"]
["","EER","","","3.03","2.91"]
["","COP","","","3.10","3.21"]
["","Energy labeling Directive","Cooling","","B","C"]
["","","Heating","","D","C"]
["Heating capacity","Nom.","","kW","5.80","7.00"]
["","Min.","","kW","1.70","1.70"]
["","Max.","","kW","6.00","8.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]