{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25K3V1B","FDXS35F2VEB / RXS35K2V1B","FDXS50F2VEB / RXS50K2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.4 (2)","3.4 (2)","5.0 (2)"]
["Space cooling","SEER","","","5.08","4.82","5.12"]
["","Annual energy consumption","","kWh/a","165","247","342"]
["","Capacity","Pdesign","kW","2.40","3.40","5.00"]
["","Energy efficiency class","","","B","B","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.60","2.90","3.50"]
["","SCOP/A","","","4.19","3.81","3.41"]
["","Energy efficiency class","","","A+","A","A"]
["","Annual energy consumption","","kWh/a","869","1,066","1,438"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","EER","","","3.72 (1)","3.21 (1)","3.03 (1)"]
["","Annual energy consumption","","kWh","323","530","825"]
["","COP","","","3.90 (1)","3.39 (1)","3.10 (1)"]
["","Energy labeling Directive","Cooling","","A","A","B"]
["","","Heating","","A","C","D"]
["Heating capacity","Nom.","","kW","3.2 (3)","4.0 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","4.5","5.0","6.0"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]