{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-K"]
[]
[]
[]
[]
["","","","","FFQ25B9V1B / RXS25K2V1B","FFQ25B9V1B / RXS25K3V1B","FFQ35B9V1B / RXS35K2V1B","FFQ50B9V1B / RXS50K2V1B"]
["Cooling capacity","Nom.","","kW","2.50 (3)","2.50 (3)","3.4 (3)","4.7 (3)"]
["Space cooling","SEER","","","","4.36","4.53","5.14"]
["","Annual energy consumption","","kWh/a","","201","270","334"]
["","Capacity","Pdesign","kW","","2.50","3.50","4.90"]
["","Energy efficiency class","","","","C","C","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","2.80","2.90","4.50"]
["","SCOP/A","","","","3.75","3.49","3.41"]
["","Energy efficiency class","","","","A","A","A"]
["","Annual energy consumption","","kWh/a","","1,046","1,162","1,847"]
["Piping connections","Liquid","OD","mm","","","6.35","6.35"]
["","Gas","OD","mm","","","9.5","12.7"]
["","Drain","OD","mm","","","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","EER","","","3.43","3.43","2.62","2.61"]
["","Annual energy consumption","","kWh","365","365","650","900"]
["","COP","","","3.48","3.48","2.81","2.81"]
["","Energy labeling Directive","Cooling","","A","A","D","D"]
["","","Heating","","B","B","D","D"]
["Heating capacity","Nom.","","kW","3.20 (4)","3.20 (4)","4.5 (4)","5.5 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]