{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 2MXM-M9"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / 2MXM50M3V1B9","FTXM20N2V1B / FTXM25N2V1B / 2MXM50M3V1B9","FTXM20N2V1B / FTXM35N2V1B / 2MXM50M3V1B9","FTXM25N2V1B / FTXM25N2V1B / 2MXM50M3V1B9","FTXM25N2V1B / FTXM42N2V1B / 2MXM50M3V1B9","FTXM25N2V1B / FTXM50N2V1B / 2MXM50M3V1B9","FTXM35N2V1B / FTXM42N2V1B / 2MXM50M3V1B9","FTXM42N2V1B / FTXM42N2V1B / 2MXM50M3V1B9"]
["Cooling capacity","Nom.","","kW","4.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00"]
["Space cooling","SEER","","","8.71","8.67","8.54","8.53","8.58","8.52","8.60","8.56"]
["","Annual energy consumption","","kWh/a","161","182","205","205","204","206","204","205"]
["","Capacity","Pdesign","kW","4.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.00","4.10","4.20","4.20","4.20","4.20","4.20","4.20"]
["","SCOP/A","","","4.61","4.61","4.61","4.61","4.65","4.71","4.67","4.70"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","3.27","3.33","3.40","3.40","3.42","3.53","3.43","3.44"]
["","Annual energy consumption","","kWh/a","1,214","1,244","1,275","1,275","1,265","1,249","1,258","1,251"]
["Nominal efficiency","Annual energy consumption","","kWh","471","534","619","623","611","605","604","601"]
["","EER","","","4.25","4.21","4.04","4.01","4.09","4.13","4.14","4.16"]
["","COP","","","4.09","4.10","4.12","4.08","4.03","3.98","4.00","3.98"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","5.20","5.60","5.60","5.60","5.60","5.60","5.60","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]