{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 5MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM25N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90A2V1B9","FTXM42N2V1B / FTXM50N2V1B / 5MXM90A2V1B9","FTXM20N2V1B / FTXM71N2V1B / 5MXM90A2V1B9","FTXM20N2V1B / FTXM20N2V1B / FTXM50N2V1B / 5MXM90A2V1B9","FTXM20N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90A2V1B9","FTXM20N2V1B / FTXM35N2V1B / FTXM35N2V1B / 5MXM90A2V1B9","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 5MXM90A2V1B9"]
["Cooling capacity","Nom.","","kW","8.00","8.00","8.00","8.00","8.00","8.00","7.80"]
["Heating capacity","Nom.","","kW","10.00","10.00","10.00","10.00","10.00","10.00","10.00"]
["Nominal efficiency","EER","","","3.72","3.34","3.33","3.82","3.71","3.73","4.15"]
["","COP","","","4.09","3.74","3.69","4.28","4.08","3.99","4.58"]
["","Annual energy consumption","","kWh","1075","1199","1202","1047","1077","1073","940"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","8.00","8.00","8.00","8.00","8.00","8.00","7.80"]
["","SEER","","","7.18","6.85","6.84","7.29","7.17","7.18","7.55"]
["","Annual energy consumption","","kWh/a","391","411","410","387","391","392","366"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","5.60","5.20","4.50","6.46","5.60","6.46","6.46"]
["","SCOP/A","","","4.36","4.21","4.26","4.34","4.35","4.20","4.50"]
["","Pdh Heating capacity at -10°","","kW","4.48","4.19","3.84","4.98","4.47","4.97","5.02"]
["","Annual energy consumption","","kWh/a","1799","1731","1478","2083","1803","2152","2010"]