{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60F3V1B","FTXS60GV1B / RXS60F4V1B","FTXS71GV1B / RXS71FAV1B9","FTXS71GV1B / RXS71FAV1B"]
["Cooling capacity","Min.","","kW","1.7","1.7","2.3","2.3"]
["","Max.","","kW","6.7","6.7","8.5","8.5"]
["","Nom.","","kW","6.0 (3)","6.0 (2)","7.1 (2)","7.1 (3)"]
["Space cooling","SEER","","","","5.35","5.23"]
["","Annual energy consumption","","kWh/a","","393","475"]
["","Capacity","Pdesign","kW","","6.00","7.10"]
["","Energy efficiency class","","","","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","4.80","6.50"]
["","SCOP/A","","","","3.75","3.50"]
["","Energy efficiency class","","","","A","A"]
["","Annual energy consumption","","kWh/a","","1,790","2,593"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","12.7","12.7","15.9","15.9"]
["","Drain","OD","mm","18.0","18.0","18.0","18.0"]
["Nominal efficiency","EER","","","3.02","3.02","3.02","3.02"]
["","Annual energy consumption","","kWh","995","995","1,175","1,175"]
["","COP","","","3.43","3.43","3.22","3.22"]
["","Energy labeling Directive","Cooling","","B","B","B","B"]
["","","Heating","","B","B","C","C"]
["Heating capacity","Nom.","","kW","7.0 (4)","7.0 (3)","8.2 (3)","8.2 (4)"]
["","Min.","","kW","1.7","1.7","2.3","2.3"]
["","Max.","","kW","8.0","8.0","10.2","10.2"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]