{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":14,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / 4MXS-E"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / FTXS20K2V1B / FTXS20K2V1B / FTXS20K2V1B / 4MXS80E3V3B2","FTXS20K2V1B / FTXS20K2V1B / FTXS20K2V1B / FTXS20K2V1B / 4MXS80E3V3B","FTXS20K2V1B / FTXS20K2V1B / FTXS42K2V1B / 4MXS80E3V3B2","FTXS20K2V1B / FTXS25K2V1B / FTXS35K2V1B / 4MXS80E3V3B","FTXS35K2V1B / FTXS42K2V1B / 4MXS80E3V3B","FTXS20K2V1B / FTXS20K2V1B / FTXS42K2V1B / 4MXS80E3V3B","FTXS42K2V1B / FTXS42K2V1B / 4MXS80E3V3B2","FTXS35K2V1B / FTXS42K2V1B / 4MXS80E3V3B2","FTXS20K2V1B / FTXS25K2V1B / FTXS35K2V1B / 4MXS80E3V3B2","FTXS42K2V1B / FTXS42K2V1B / 4MXS80E3V3B"]
["Space cooling","Annual energy consumption","","kWh/a","407","407","425","423","458","425","468","458","423","468"]
["","Energy efficiency class","","","A++","A++","A+","A+","A","A+","A","A","A+","A"]
["","Capacity","Pdesign","kW","7.32","7.32","7.35","7.31","7.24","7.35","7.40","7.24","7.31","7.40"]
["","SEER","","","6.31","6.31","6.06","6.05","5.53","6.06","5.54","5.53","6.05","5.54"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","2,194","2,194","1,919","1,921","1,572","1,919","1,591","1,572","1,921","1,591"]
["","Capacity","Pdesign","kW","6.23","6.23","5.32","5.33","4.30","5.32","4.34","4.30","5.33","4.34"]
["","Energy efficiency class","","","A","A","A","A","A","A","A","A","A","A"]
["","SCOP/A","","","3.98","3.98","3.88","3.88","3.83","3.88","3.82","3.83","3.88","3.82"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]