{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ125CVEB"]
["Sound pressure level","Heating","High","dBA","47"]
["","","Nom.","dBA","43"]
["","","Low","dBA","40"]
["","Cooling","Low","dBA","40"]
["","","High","dBA","47"]
["","","Nom.","dBA","43"]
["Standard Accessories","Installation manual","","","Installation manual"]
["","Operation manual","","","Operation manual"]
["","Declaration of conformity","","","Declaration of conformity"]
["","Drain hose","","","Drain hose"]
["","Clamp metal","","","Clamp metal"]
["","Washer for hanger bracket","","","Washer for hanger bracket"]
["","Clamps","","","Clamps"]
["","Washer clamp","","","Washer clamp"]
["","Joint insulation & Sealing material","","","Joint insulation & Sealing material"]
["","Elbow","","","Elbow"]
["","Installation pattern","","","Installation pattern"]
["","Blocking material","","","Blocking material"]
["","L-bent piping","","","L-bent piping"]
["","Screws","","","Screws"]
["","Non woven fabric","","","Non woven fabric"]
["Control systems","Wired remote control","","","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58"]
["Piping connections","Liquid","OD","mm","9.52"]
["","Gas","OD","mm","15.9"]
["","Drain","","","VP25 (OD Ø32.0)"]
["Sound power level","Cooling","","dBA","65"]
["","Heating","","dBA","65"]
["Dimensions","Unit","Width","mm","950"]
["","","Depth","mm","950"]
["","","Height","mm","198"]
["Casing","Material","","","Resin"]
["","Colour","","","Fresh White"]
["Weight","Unit","","kg","26"]
["Drain-up height","mm","","","600"]
["Power supply","Phase","","","1~"]
["","Name","","","VE"]
["","Frequency","","Hz","50/60"]
["","Voltage","","V","220-240/220"]