{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":11,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Sound pressure level","Heating","","High","dBA","49","","","52"]
["","","","Low","dBA","46","","","49"]
["","Cooling","","Low","dBA","46","","","49"]
["","","","High","dBA","49","","","52"]
["Standard Accessories","Drain socket","","","","1","","1","1","","1"]
["","Installation manual","","","","1","Installation manual","1","1","Installation manual","1"]
["Refrigerant","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Charge","","","kg","1.5","","","2.3"]
["","Type","","","","R-410A","","","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","m","20","","","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","","","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","825","","","900"]
["","","","Depth","mm","300","","","320"]
["","","","Height","mm","735","","","770"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Frequency","","","Hz","50","","","50"]
["","Voltage","","","V","220-240","","","220-240"]
["Notes","","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220V","","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220V"]
["","","","","","(2) - Contains fluorinated greenhouse gases","(2) - 230V","","(2) - Contains fluorinated greenhouse gases","(2) - 230V"]
["Dimensions","Unit","","Height","mm","","735","735","","770","770"]
["","","","Width","mm","","825","825","","900","900"]
["","","","Depth","mm","","300","300","","320","320"]
["Weight","Unit","","","kg","","48","48","","71","71"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Max.","°CDB","","46","46","","46","46"]
["","Heating","Ambient","Min.","°CWB","","-15","-15","","-15","-15"]
["","","","Max.","°CWB","","18","20","","18","20"]
["Sound pressure level","Cooling","","High","dBA","","49","49","","52","52"]
["","","","Low","dBA","","46","46","","49","49"]
["","Heating","","High","dBA","","49","49","","52","52"]
["","","","Low","dBA","","46","46","","49","49"]
["Refrigerant","Type","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Charge","","","kg","","1.5","1.5","","2.3","2.3"]
["","Charge","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","","30","30","","30","30"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","","20","20","","20","20"]
["Standard Accessories","Drain plug","","","","","Drain plug","","","Drain plug"]
["Power supply","Phase","","","","","1~","1~","","1~","1~"]
["","Frequency","","","Hz","","50","50","","50","50"]
["","Voltage","","","V","","220-240","220-240","","220-240","220-240"]
["Notes","","","","","","(3) - 240V","","","(3) - 240V"]
["Sound power level","Cooling","","","dBA","","","","65"]