{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":71,"n_cols":11,"rows_kept":71,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Sound pressure level","Heating","","High","dBA","47","47","48","48"]
["","Cooling","","High","dBA","46","46","48","48"]
["Standard Accessories","Drain cap","","","","1","1","","1"]
["","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","Multilingual fluorinated greenhouse gases labels"]
["Refrigerant","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.0","1.20","1.3"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","Super low","rpm","780","780","780","790"]
["","","Heating","Super low","rpm","740","740","740","780"]
["Operation range","Cooling","Ambient","Max.","°CDB","46","46","46","46"]
["","","","Min.","°CDB","-10","-10","-10","-10"]
["","Heating","Ambient","Max.","°CWB","18","18","18","18"]
["","","","Min.","°CWB","-15","-15","-15","-15"]
["Piping connections","Level difference","IU - OU","Max.","m","","","15"]
["","Additional refrigerant charge","","","kg/m","","","0.020 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","765","765","765","765"]
["","","","Depth","mm","285","285","285","285"]
["","","","Height","mm","550","550","550","550"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","34","34","34","39"]
["Fan","Air flow rate","Heating","Super low","cfm","904","904","904","960"]
["","","","Super low","m³/min","25.6","25.6","25.6","27.2"]
["","","Cooling","Super low","m³/min","30.1","30.1","30.1","30.6"]
["","","","Super low","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Drain plug","","","","","","1","","1","1"]
["Fan","Air flow rate","Cooling","Super low","m³/min","","","","","48.9","45.0"]
["","","Heating","Super low","m³/min","","","","","43.1","46.3"]
["","","","Super low","cfm","","","","","1727","1589"]
["","","Heating","Super low","cfm","","","","","1522","1635"]
["Dimensions","Unit","","Height","mm","","","","","735","735"]
["","","","Width","mm","","","","","825","825"]
["","","","Depth","mm","","","","","300","300"]
["Weight","Unit","","","kg","","","","","47","48"]
["Fan motor","Speed","Cooling","Super low","rpm","","","","","670"]
["","","Heating","Super low","rpm","","","","","670"]
["Compressor","Type","","","","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","","","-10","-10"]
["","","","Max.","°CDB","","","","","46","46"]
["","Heating","Ambient","Min.","°CWB","","","","","-15","-15"]
["","","","Max.","°CWB","","","","","18","18"]
["Sound pressure level","Cooling","","High","dBA","","","","","48","49"]
["","","","Low","dBA","","","","","44","46"]
["","Heating","","High","dBA","","","","","48","49"]
["","","","Low","dBA","","","","","45","46"]
["Refrigerant","Type","","","","","","","","R-410A","R-410A"]
["","Charge","","","kg","","","","","1.7","1.5"]
["","Charge","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","","","","","30","30"]
["","Additional refrigerant charge","","","kg/m","","","","","0.020 (for piping length exceeding 10m)","0.020 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","","","","","20.0","20"]
["Power supply","Phase","","","","","","","","1~","1~"]
["","Frequency","","","Hz","","","","","50","50"]
["","Voltage","","","V","","","","","220-230-240","220-230-240"]
["Notes","","","","","","","","","","(1) - 230V"]