{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":26,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXYTQ-UYF"]
[]
[]
[]
[]
["","","","","","RXYTQ8U7YF","RXYTQ10U7YF","RXYTQ12U7YF","RXYTQ14U7YF","RXYTQ16U7YF","RXYTQ18U7YF","RXYTQ20U7YF","RXYTQ22U7YF","RXYTQ24U7YF","RXYTQ26U7YF","RXYTQ28U7YF","RXYTQ30U7YF","RXYTQ32U7YF","RXYTQ34U7YF","RXYTQ36U7YF","RXYTQ38U7YF","RXYTQ40U7YF","RXYTQ42U7YF","RXYTQ44U7YF","RXYTQ46U7YF","RXYTQ48U7YF"]
["System","Outdoor unit module 1","","","","","","","","","RXYTQ8U","RXYTQ8U","RXYTQ10U","RXYTQ8U","RXYTQ12U","RXYTQ12U","RXYTQ14U","RXYTQ16U","RXYTQ8U","RXYTQ8U","RXYTQ8U","RXYTQ10U","RXYTQ10U","RXYTQ12U","RXYTQ14U","RXYTQ16U"]
["","Outdoor unit module 2","","","","","","","","","RXYTQ10U","RXYTQ12U","RXYTQ12U","RXYTQ16U","RXYTQ14U","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ10U","RXYTQ12U","RXYTQ14U","RXYTQ14U","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ16U"]
["","Outdoor unit module 3","","","","","","","","","","","","","","","","","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ16U","RXYTQ16U"]
["Capacity range","HP","","","","8","10","12","14","16","18","20","22","24","26","28","30","32","34","36","38","40","42","44","46","48"]
["Maximum number of connectable indoor units","","","","","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)","64 (9)"]
["Indoor index connection","Min.","","","","100","125","150","175","200","225","250","275","300","325","350","375","400","425","450","475","500","525","550","575","600"]
["","Nom.","","","","200","250","300","350","400","450","500","550","600","650","700","750","800","850","900","950","1,000","1,050","1,100","1,150","1,200"]
["","Max.","","","","260","325","390","455","520","585","650","715","780","845","910","975","1,040","1,105","1,170","1,235","1,300","1,365","1,430","1,495","1,560"]
["Dimensions","Unit","","Height","mm","1,685","1,685","1,685","1,685","1,685"]
["","","","Width","mm","930","1,240","1,240","1,240","1,240"]
["","","","Depth","mm","765","765","765","765","765"]
["Weight","Unit","","","kg","198","234","234","283","283"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","162","223","223","260","260"]
["","","","Nom.","cfm","5,721","7,875","7,875","9,182","9,182"]
["","External static pressure","","Max.","Pa","78","78","78","78","78"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Operation range","Cooling","","Min.","°CDB","-5.0","-5.0","-5.0","-5.0","-5.0"]
["","","","Max.","°CDB","52.0","52.0","52.0","52.0","52.0"]
["","Heating","","Min.","°CWB","-20.0","-20.0","-20.0","-20.0","-20.0"]
["","","","Max.","°CWB","15.5","15.5","15.5","15.5","15.5"]
["Sound power level","Cooling","","Nom.","dBA","78.0 (10)","79.2 (10)","81.0 (10)","81.6 (10)","86.0 (10)","81.7 (10)","82.8 (10)","83.2 (10)","86.6 (10)","84.3 (10)","87.2 (10)","87.3 (10)","89.0 (10)","87.4 (10)","87.7 (10)","87.8 (10)","88.0 (10)","89.4 (10)","89.6 (10)","89.7 (10)","90.8 (10)"]
["Sound pressure level","Cooling","","Nom.","dBA","57.0 (11)","59.0 (11)","61.0 (11)","61.0 (11)","64.0 (11)","61.1 (11)","62.5 (11)","63.1 (11)","64.8 (11)","64.0 (11)","65.8 (11)","65.8 (11)","67.0 (11)","65.8 (11)","66.3 (11)","66.3 (11)","66.6 (11)","67.6 (11)","68.0 (11)","68.0 (11)","68.8 (11)"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","6.7","10.3","10.4","11.7","11.8"]
["Piping connections","Liquid","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","","","OD","mm","9.52","9.52","12.7","12.7","12.7"]
["","Gas","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","","","OD","mm","19.1","22.2","28.6","28.6","28.6"]
["","Total piping length","System","Actual","m","1,000 (12)","1,000 (12)","1,000 (12)","1,000 (12)","1,000 (12)"]
["Power supply","Name","","","","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF","YF"]
["","Phase","","","","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400"]
["Notes","","","","","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 27°CDB (26,7°CDB for Kuwait), 19,0°CWB (19,4°CWB for Kuwait), outdoor tem. 35°CDB, AHRI 1230:2010, power input indoor units (duct type) included"]
["","","","","","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included","(2) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011, power input indoor units (duct type) included"]
["","","","","","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included","(3) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB, AHRI 1230:2010, power input indoor units (duct type) included"]
["","","","","","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011","(4) - Cooling: T3: indoor temp. 29.0°CDB, 19.0°CWB, outdoor temp. 46°CDB, ISO15042:2011"]
["","","","","","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011","(5) - Cooling: T1: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 35°CDB, ISO15042:2011"]
["","","","","","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011","(6) - Cooling: indoor temp. 27.0°CDB, 19.0°CWB, outdoor temp. 29°CDB, ISO15042:2011"]
["","","","","","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level differrence: 0m. Power input of indoor units (duct type) included"]
["","","","","","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019","(8) - Cooling seasonal performance factor for hot climates at T3 condition per ISO 16358-1:2013/AMD 1:2019"]
["","","","","","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(9) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%)."]
["","","","","","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates.","(10) - Sound power level is an absolute value that a sound source generates."]
["","","","","","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(11) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual","(12) - Refer to refrigerant pipe selection or installation manual"]
["","","","","","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(13) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C","(14) - RLA is based on following conditions: indoor temp. 29°CDB, 19°CWB; outdoor temp. 46°C"]
["","","","","","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(15) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current."]
["","","","","","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(16) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current."]
["","","","","","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(17) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan","(18) - FLA means the nominal running current of the fan"]
["","","","","","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%.","(19) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(20) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room.","(21) - Sound values are measured in a semi-anechoic room."]
["","","","","","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(22) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA"]
["","","","","","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual","(23) - For detailed contents of standard accessories, see installation/operation manual"]
["","","","","","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination","(24) - Multi combination (18~48HP) data is corresponding with the standard multi combination"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Connection pipes","","","","1","1","1","1","1"]