{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC073"]
[]
[]
[]
[]
["","","","","BRC073A1"]
["Packing","Material","","","Carton_"]
["","Weight","","kg","0.050"]
["Ambient temperature","الرطوبة النسبية <","","%","95"]
["","Storage","Min.","درجة مئوية","-20"]
["","","Max.","درجة مئوية","70"]
["","Operation","Min.","درجة مئوية","-10"]
["","","Max.","درجة مئوية","50"]
["إعداد درجة الحرارة","الدقة","","درجة مئوية","1"]
["","نطاق نقطة التعيين","التبريد","درجة مئوية","18-32"]
["","","التسخين","درجة مئوية","10-30"]
["Dimensions","الوحدة المعبأة","العرض","mm","220"]
["","","الارتفاع","mm","50"]
["","","العمق","mm","160"]
["","Unit","العرض","mm","120"]
["","","العمق","mm","19"]
["","","الارتفاع","mm","120"]
["الغلاف","غطاء الزر","","","لا"]
["","اللون","","","أبيض صاف"]
["","ضوء التشغيل","اللون","","أخضر"]
["شاشة LCD","النوع","","","نقطة كاملة (160 × 255)"]
["","إضاءة خلفية","اللون","","أبيض"]
["","الأبعاد","العرض","mm","68.85"]
["","","الارتفاع","mm","43.2"]
["الوزن","الوحدة المعبأة","","kg","0.348"]
["","الوحدة","","kg","0.290"]