{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Sound pressure level","Heating","High","ديسيبل أمبير","36","37","37","38"]
["","","Nom.","ديسيبل أمبير","34","35","35","36"]
["","","متوسط","ديسيبل أمبير","31","32","33","34"]
["","Cooling","متوسط","ديسيبل أمبير","34","35","35","36"]
["","","Low","ديسيبل أمبير","31","32","33","34"]
["","","High","ديسيبل أمبير","36","37","37","38"]
["Standard Accessories","أنبوب العزل الحراري","","","2","2","2","2"]
["","مادة مشبك السلك","","","7","7","7","7"]
["","حلقة تثبيت الخرطوم","","","1","1","1","1"]
["","خرطوم الصرف","","","1","1","1","1"]
["","حلقة إحكام الربط","","","8","8","8","8"]
["","لبادة مانعة للتسريب (كبيرة)","","","1","1","1","1"]
["","لبادة مانعة للتسريب (صغيرة)","","","1","1","1","1"]
["","تثبيت بالراتنج","","","1","1","1","1"]
["","مسامير لولبية","","","2","2","2","2"]
["","مثبتات الأسلاك","","","2","2","2","2"]
["أنظمة التحكم","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","9.52"]
["","غاز","القطر الخارجي","mm","9.50","12.7","12.7","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20"]
["Sound power level","التبريد","","ديسيبل أمبير","53","54","54","55"]
["Dimensions","Unit","العرض","mm","960","960","1,270","1,270"]
["","","العمق","mm","690","690","690","690"]
["","","الارتفاع","mm","235","235","235","235"]
["الغلاف","المادة","","","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية"]
["","اللون","","","White","White","White","White"]
["الوزن","الوحدة","","kg","24.0","25.0","31.0","32.0"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]