{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","40","","","","","","45"]
["","","","Silent operation","ديسيبل أمبير","19","","","","","","22"]
["","","","Low","ديسيبل أمبير","27","","","","","","33"]
["","Cooling","","Silent operation","ديسيبل أمبير","19","","","","","","21"]
["","","","Low","ديسيبل أمبير","24","","","","","","33"]
["","","","High","ديسيبل أمبير","40","","","","","","45"]
["","","","Nom.","ديسيبل أمبير","34","","","","","","39"]
["","Cooling","","Nom.","ديسيبل أمبير","32","","","","","","39"]
["Standard Accessories","دليل التركيب","","","","1","","","","","","1"]
["","دليل التشغيل","","","","1","","","","","","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","","","","","","1"]
["","البطاريات","","","","2","","","","","","2"]
["","حامل جهاز التحكم عن بعد","","","","1","","","","","","1"]
["","لوح التثبيت","","","","1","","","","","","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","","","","","","2"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","","","","","","2"]
["أنظمة التحكم","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Piping connections","Liquid","","القطر الخارجي","مم","6.35","","","","","","6.35"]
["","غاز","","القطر الخارجي","مم","9.5","","","","","","9.5"]
["","Drain","","","","18","","","","","","18"]
["Power input","Cooling","","Nom.","كيلوواط","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Heating","","Nom.","كيلوواط","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","التبريد","","","ديسيبل أمبير","58","","","","","","59"]
["","التدفئة","","","ديسيبل أمبير","58","","","","","","59"]
["Dimensions","Unit","","العرض","مم","780","","","","","","900"]
["","","","العمق","مم","215","","","","","","215"]
["","","","الارتفاع","مم","289","","","","","","298"]
["الغلاف","اللون","","","","White","","","","","","White"]
["الوزن","الوحدة","","","كغ","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Frequency","","","Hz","50","","","","","","50"]
["","الاسم","","","","V1","","","","","","V1"]
["","Voltage","","","V","220-240","","","","","","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 220 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 230 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["Power input","Cooling","","Nom.","كيلوواط","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Heating","","Nom.","كيلوواط","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["الغلاف","اللون","","","","","أبيض","أبيض","أبيض","أبيض","أبيض","","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","مم","","215","289","215","298","215","","215","298","215"]
["","","","العرض","مم","","780","780","780","900","900","","900","900","900"]
["","","","العمق","مم","","289","215","289","215","298","","298","215","298"]
["الوزن","الوحدة","","","كغ","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Fan","Air flow rate","التبريد","High","م³/دقيقة","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","م³/دقيقة","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["Fan","Air flow rate","التبريد","Low","م³/دقيقة","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Silent operation","م³/دقيقة","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","التدفئة","High","م³/دقيقة","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","م³/دقيقة","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["Fan","Air flow rate","التدفئة","Low","م³/دقيقة","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Silent operation","م³/دقيقة","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","","58","58","58","59","59","","59","60","60"]
["","التدفئة","","","ديسيبل أمبير","","58","58","58","59","59","","59","60","60"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","","40","41","41","45","45","","45","46","46"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","","32","33","33","","37","","39","","40"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","","24","25","25","29","29","","33","34","34"]
["","","","Silent operation","ديسيبل أمبير","","19","19","19","19","19","","21","23","23"]
["","Heating","","High","ديسيبل أمبير","","40","41","41","45","45","","45","47","47"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","","34","34","34","","39","","39","","40"]
["Sound pressure level","Heating","","Low","ديسيبل أمبير","","27","27","27","29","29","","33","34","34"]
["","","","Silent operation","ديسيبل أمبير","","19","19","19","19","19","","22","24","24"]
["وصلات الأنابيب","سائل","","القطر الخارجي","مم","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","مم","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","التصريف","","","","","18","18","18","18","18","","18","18","18"]
["أنظمة التحكم","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standard Accessories","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","الطور","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Voltage","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Fan","Air flow rate","التبريد","Nom.","م³/دقيقة","","","9.1","","11.2","","","","11.9"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","","","33","","37","","","","40"]
["Fan","Air flow rate","التدفئة","Nom.","م³/دقيقة","","","8.0","","9.3","","","","10.8"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","","","34","","39","","","","40"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standard Accessories","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Notes","","","","","","","","","","","(4) - 240 فولت"]