{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Sound pressure level","Heating","High","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Low","dBA","38","44","46","48"]
["","Cooling","Low","dBA","38","44","46","48"]
["","","High","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","دعامة للتركيب","","","دعامة للتركيب","دعامة للتركيب","دعامة للتركيب","دعامة للتركيب"]
["","مطاط حماية الفتحات","","","مطاط حماية الفتحات","مطاط حماية الفتحات","مطاط حماية الفتحات","مطاط حماية الفتحات"]
["","كم وصل","","","كم وصل","كم وصل","كم وصل","كم وصل"]
["","عازل لأدوات التثبيت","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["","غطاء","","","غطاء","غطاء","غطاء","غطاء"]
["","مشابك","","","مشابك","مشابك","مشابك","مشابك"]
["","مسامير لولبية","","","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","نموذج التركيب","","","نموذج التركيب","نموذج التركيب","نموذج التركيب","نموذج التركيب"]
["","مادة حماية من الندى","","","مادة حماية من الندى","مادة حماية من الندى","مادة حماية من الندى","مادة حماية من الندى"]
["","تمديدات سلكية للتحكم عن بعد","","","تمديدات سلكية للتحكم عن بعد","تمديدات سلكية للتحكم عن بعد","تمديدات سلكية للتحكم عن بعد","تمديدات سلكية للتحكم عن بعد"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Power input","Cooling","Nom.","كيلو واط","0.117","0.238","0.238","0.276"]
["","Heating","Nom.","كيلو واط","0.117","0.238","0.238","0.276"]
["مستوى طاقة الصوت","التبريد","","dBA","55","62","63","65"]
["","التدفئة","","dBA","55","62","63","65"]
["Dimensions","Unit","العرض","mm","600","600","600","600"]
["","","العمق","mm","270","350","350","350"]
["","","الارتفاع","mm","1,850","1,850","1,850","1,850"]
["الغلاف","اللون","","","أبيض صاف","أبيض صاف","أبيض صاف","أبيض صاف"]
["الوزن","الوحدة","","kg","39","47","47","47"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","فولت","220-240/220","220-240/220","220-240/220","220-240/220"]